; This is the Setup information file to install hardware components
; Copyright (c) 2002 3Com Corporation
 
[version]
signature				="$CHICAGO$"
Compatible				= 1
Class					= Net
ClassGUID				= {4D36E972-E325-11CE-BFC1-08002BE10318}
provider				= %V_MS%
CatalogFile 				= w9x90xbc.cat
DriverVer                               = 06/04/2003,04.41.0000.0

[Manufacturer]
%V_3COM%				= 3COM

[SourceDisksNames]
50					= %Source_Disk_Name%,,,

[SourceDisksFiles]
el90xBC5.sys				= 50 
;el90xBC4.sys				= 50 
;el90xBC3.sys				= 50
;netdi90x.dll				= 50

[ControlFlags]
ExcludeFromSelect.NT			= *

[3COM]
%PCI\VEN_10b7&DEV_9200&SUBSYS_100010B7.DeviceDesc%	= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_100010B7
%PCI\VEN_10b7&DEV_9200&SUBSYS_700010B7.DeviceDesc%	= PCIEL905CTXMH.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_700010B7
%PCI\VEN_10b7&DEV_9058.DeviceDesc%			= PCIEL905CMBDLX.ndi, 	PCI\VEN_10b7&DEV_9058
%PCI\VEN_10b7&DEV_905A.DeviceDesc%			= PCIEL905AFX.ndi, 	PCI\VEN_10b7&DEV_905A 
%PCI\VEN_10b7&DEV_9055.DeviceDesc%			= PCIEL9055TX.ndi, 	PCI\VEN_10b7&DEV_9055&SUBSYS_905510b7 	
%PCI\VEN_10b7&DEV_900A.DeviceDesc%			= PCIEL900AFL.ndi, 	PCI\VEN_10b7&DEV_900A 
%PCI\VEN_10b7&DEV_9004.DeviceDesc%			= PCIEL9004TPO.ndi, 	PCI\VEN_10b7&DEV_9004 
%PCI\VEN_10b7&DEV_9005.DeviceDesc%			= PCIEL9005COMBO.ndi, 	PCI\VEN_10b7&DEV_9005 
%PCI\VEN_10b7&DEV_9006.DeviceDesc%			= PCIEL9006TPC.ndi, 	PCI\VEN_10b7&DEV_9006

;*** 3Com 3C920 and 3C918 Controller based integrated Ethernet ***
%PCI\VEN_10b7&DEV_9201&SUBSYS_12B8103C.DeviceDesc%	= PCIEL905CTXMB.ndi, 	PCI\VEN_10b7&DEV_9201&SUBSYS_12B8103C
%PCI\VEN_10b7&DEV_9201&SUBSYS_233C1106.DeviceDesc%	= PCIEL905CTXMB.ndi, 	PCI\VEN_10b7&DEV_9201&SUBSYS_233C1106
%PCI\VEN_10b7&DEV_9201&SUBSYS_B00F144D.DeviceDesc%	= PCIEL905CTXMB.ndi, 	PCI\VEN_10b7&DEV_9201&SUBSYS_B00F144D
%PCI\VEN_10b7&DEV_9201.DeviceDesc%			= PCIEL905CTXMB.ndi, 	PCI\VEN_10b7&DEV_9201
%PCI\VEN_10b7&DEV_9202.DeviceDesc%			= PCIEL905CTXWNM.ndi, 	PCI\VEN_10b7&DEV_9202
%PCIEL9200LOM1246103C.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_1246103C
%PCIEL9200LOM1247103C.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_1247103C
%PCIEL9200LOM1248103C.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_1248103C
%PCIEL9200LOM211914A4.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_211914A4
%PCIEL9200LOM303C1462.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_303C1462
%PCIEL9200LOM1101144D.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_1101144D
%PCIEL9200LOM802A1043.DeviceDesc%			= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_802A1043
%PCIEL9055LOM.DeviceDesc%				= PCIEL9055TX.ndi, 	PCI\VEN_10b7&DEV_9055
%MOBILEEL9200LOM00E3.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00E31028
%MOBILEEL9200LOM00E4.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00E41028
%MOBILEEL9200LOM00C8.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00C81028
%MOBILEEL9200LOM00D4.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00D41028
%MOBILEEL9200LOM00D5.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00D51028
%MOBILEEL9200LOM00B8.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00B81028
%MOBILEEL9200LOM00B9.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00B91028
%MOBILEEL9200LOM012A.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_012A1028
%MOBILEEL9200LOM012B.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_012B1028
%MOBILEEL9200LOM0122.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_01221028
%MOBILEEL9200LOM00F3.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00F31028
%MOBILEEL9200LOM00F4.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_00F41028
%MOBILEEL9200LOMC002.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_C002144D
%MOBILEEL9200LOMC005.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_C005144D
%MOBILEEL9200LOM3500.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_3500107B
%MOBILEEL9200LOM0013.DeviceDesc%			= MOBILEEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200&SUBSYS_001314C0
%PCIEL9200LOM.DeviceDesc%				= PCIEL905CTXM.ndi, 	PCI\VEN_10b7&DEV_9200


;*** WIN 9X EXLCUSIVE *************************************************************


[PCIEL905CTXMB.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
DelReg		= EL90x.Old
AddReg		= PCIEL905CTXMB.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDet, EnhLANPwrMgmt, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL905CTXWNM.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
DelReg		= EL90x.Old
AddReg		= PCIEL905CTXWNM.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDet, EnhLANPwrMgmt, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL905CTXM.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
DelReg		= EL90x.Old
AddReg		= PCIEL905CTXM.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDet, EnhLANPwrMgmt, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[MOBILEEL905CTXM.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
DelReg		= EL90x.Old
AddReg		= PCIEL905CTXM.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDetMOBILE, EnhLANPwrMgmtMOBILE, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL905CTXMH.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
DelReg		= EL90x.Old
AddReg		= PCIEL905CTXMH.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDet, EnhLANPwrMgmt, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL905CMBDLX.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL905CMBDLX.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.CMBDLX, FLOWCONTROL, downPollRate, InitDelayCount, DoubleNego, PHYCompat, LnkChk, SWCblDet, EnhLANPwrMgmt, RWUMAGIC, RWUARP, RWUPING, STBYMAGIC, STBYPATTERN, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL905AFX.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL905AFX.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.fx, FLOWCONTROL, downPollRate, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL9055TX.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL9055TX.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tx, FLOWCONTROL, downPollRate, checksum, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL900AFL.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL900AFL.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.fl, FLOWCONTROL, downPollRate, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL9004TPO.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL9004TPO.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tpo, FLOWCONTROL, downPollRate, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL9005COMBO.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL9005COMBO.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.combo, FLOWCONTROL, downPollRate, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

[PCIEL9006TPC.ndi]
DriverVer	= 06/04/2003,04.41.0000.0
AddReg		= PCIEL9006TPC.ndi.reg,EL90x.ndi.reg,8021psupport,EL90x.params.tpc, FLOWCONTROL, downPollRate, DriverInfoAddReg
CopyFiles	= EL90x.ndis3.CopyFiles, EL90x.ndi.CopyFiles, EL90x.ndis95.CopyFiles 

;------------------------------------

[PCIEL905CTXMB.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9201"

[PCIEL905CTXWNM.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9202"

[PCIEL905CTXM.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9200&SUBSYS_100010B7"

[PCIEL905CTXMH.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9200&SUBSYS_700010B7"

[PCIEL905CMBDLX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9058"

[PCIEL905AFX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_905A"

[PCIEL9055TX.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9055"

[PCIEL900AFL.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_900A"

[PCIEL9004TPO.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9004"

[PCIEL9005COMBO.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9005"

[PCIEL9006TPC.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_10b7&DEV_9006"

;------------------------------------

[EL90x.Old]
HKR,,MediaSelect
HKR,,media
HKR,,CableHoldOffTimer
HKR,,CableToDetectTimer
HKR,,KeepPollTimer

;------------------------------------


[EL90x.ndi.reg]
HKR,,DeviceVxDs,,El90xBC3.sys
HKR,,DriverDate,,%DriverDate%
HKR,,DriverVersion,,%DriverVersion%
HKR,,ProviderName,,%ProviderName%
HKR,Ndi,NdiInstaller,,"NETDI90X.DLL, MyNdiProc"
HKR,,DevLoader,,*ndis
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"EL90x"
HKR,NDIS,MajorNdisVersion,1,00
HKR,NDIS,MinorNdisVersion,1,0A
HKR,NDIS\NDIS2,DriverName,,"EL90x$"
HKR,NDIS\ODI,DriverName,,"3C90x"
HKR,NDIS\ODI,FileName,,"3c90x.com"

HKR,Ndi\Interfaces,DefUpper,,"ndis2,ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis5,ndis4,ndis3,ndis2,odi"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

HKR,Ndi\Install,ndis3,,"EL90x.ndis3"
HKR,Ndi\Install,ndis2,,"EL90x.ndis2"
HKR,Ndi\Install,odi,,"EL90x.odi"

HKR,, InitDelayCount,,"0"
HKR,, DoubleNego,, "DISABLE"
HKR,, PHYCompat,, "ENABLE"
HKR,, PerformanceMode,, "2"

HKR,,NDIS_VERSION,,"AUTO"
HKR,NDI\params\NDIS_VERSION,,,"AUTO"
HKR,NDI\params\NDIS_VERSION,ParamDesc,,"NDIS Driver Version"
HKR,NDI\params\NDIS_VERSION,flag,1,20,00,00,00
HKR,NDI\params\NDIS_VERSION,type,,"enum"
HKR,NDI\params\NDIS_VERSION,optional,,"0"
HKR,Ndi\params\NDIS_VERSION\enum,AUTO,,"Auto Select"
HKR,Ndi\params\NDIS_VERSION\enum,NDIS4,,"NDIS 4"

HKR,,TCAUDIAG,,"TCAUM90X"
HKLM,Software\3Com\TCAUDIAG\TCAUM90X,DriverNames,,"3C90X.COM;EL90X.DOS;SYSTEM\EL90XBC3.SYS;SYSTEM\EL90XBC4.SYS;SYSTEM\EL90XBC5.SYS"

;------------------------------------

[EL90x.ndi.CopyFiles]
netdi90x.dll,,,2

;------------------------------------

[EL90x.ndis95.CopyFiles]
El90xBC5.sys,,,2
El90xBC4.sys,,,2
el90xBC3.sys,,,2

;------------------------------------

[EL90x.ndis3.CopyFiles]
El90xBC5.sys,,,2
El90xBC4.sys,,,2
el90xBC3.sys,,,2

;*** END WIN 9X EXCLUSIVE *********************************************************




;*** WIN 2K EXCLUSIVE *************************************************************

[PCIEL905CTXMB.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDet.NT, EnhLANPwrMgmt.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905CTXMB.ndi.NT.Services]
AddService     	 = EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL905CTXWNM.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDet.NT, EnhLANPwrMgmt.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905CTXWNM.ndi.NT.Services]
AddService     	 = EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL905CTXM.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDet.NT, EnhLANPwrMgmt.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905CTXM.ndi.NT.Services]
AddService     	 	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[MOBILEEL905CTXM.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDetMOBILE.NT, EnhLANPwrMgmtMOBILE.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[MOBILEEL905CTXM.ndi.NT.Services]
AddService     	 	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL905CTXMH.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDet.NT, EnhLANPwrMgmt.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905CTXMH.ndi.NT.Services]
AddService     	 	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT


[PCIEL905CMBDLX.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        	 	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT, FLOWCONTROL.NT, InitDelayCount.NT, DoubleNego.NT, PHYCompat.NT, LnkChk.NT, SWCblDet.NT, EnhLANPwrMgmt.NT, RWUMAGIC.NT, RWUARP.NT, RWUPING.NT, STBYMAGIC.NT, STBYPATTERN.NT, EL90x.params.CMBDLX.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905CMBDLX.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL905AFX.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT,EL90x.params.fx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL905AFX.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL9055TX.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        		= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT,checksum.NT,EL90x.params.tx.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL9055TX.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT


[PCIEL900AFL.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         	= 5
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT,EL90x.params.fl.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT
DelReg			= EL90x.Old.NT

[PCIEL900AFL.ndi.NT.Services]
AddService      = EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL9004TPO.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT,FLOWCONTROL.NT,EL90x.params.tpo.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL9004TPO.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL9005COMBO.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType         	= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT, FLOWCONTROL.NT,EL90x.params.combo.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL9005COMBO.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

[PCIEL9006TPC.ndi.NT]
Characteristics 	= 0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType        		= 5
DelReg			= EL90x.Old.NT
AddReg          	= EL90x.reg.NT, EL90x.software.NT, 8021psupport.NT, FLOWCONTROL.NT,EL90x.params.tpc.NT,downPollRate.NT, DriverInfoAddReg
CopyFiles		= EL90x.Driver.NT

[PCIEL9006TPC.ndi.NT.Services]
AddService      	= EL90Xbc, 2, EL90x.Service.NT, EL90x.EventLog.NT

;------------------------------------

[EL90x.Driver.NT]
el90Xbc5.SYS,,,2

;------------------------------------

[EL90x.Old.NT]
HKR,NDI\Params

;------------------------------------

[EL90x.reg.NT]
HKR, Ndi,              	Service,    	0, "EL90Xbc"
HKR, Ndi\Interfaces,    UpperRange, 	0, "ndis5"
HKR, Ndi\Interfaces,    LowerRange, 	0, "ethernet"
HKR,,TCAUDIAG,,		"TCAUM90X"
HKR,,InitDelayCount,,	"0"
HKR,,DoubleNego,,	"DISABLE"
HKR,,PHYCompat,,	"ENABLE"
HKR,,PerformanceMode,,	"2"

;------------------------------------

[EL90x.software.NT]
HKLM,Software\3Com\EL90xbc\CurrentVersion,Description,0,%ProductSoftwareDescription%
HKLM,Software\3Com\EL90xbc\CurrentVersion,MajorVersion,0x00010001,%ProductMajorVersion%
HKLM,Software\3Com\EL90xbc\CurrentVersion,MinorVersion,0x00010001,%ProductMinorVersion%
HKLM,Software\3Com\EL90xbc\CurrentVersion,Review,0x00010001,%ProductReview%
HKLM,Software\3Com\EL90xbc\CurrentVersion,ServiceName,0,%ProductSoftwareName%
HKLM,Software\3Com\EL90xbc\CurrentVersion,SoftwareType,0,%SoftwareType%
HKLM,Software\3Com\EL90xbc\CurrentVersion,Title,0,%ProductSoftwareTitle%

HKLM,Software\3Com\EL90xbc\CurrentVersion\NetRules,bindable,0x00010000,%NetRuleSoftwareBindable%
HKLM,Software\3Com\EL90xbc\CurrentVersion\NetRules,bindform,0,%NetRuleSoftwareBindForm%
HKLM,Software\3Com\EL90xbc\CurrentVersion\NetRules,class,0x00010000,%NetRuleSoftwareClass%
HKLM,Software\3Com\EL90xbc\CurrentVersion\NetRules,type,0,%NetRuleSoftwareType%
HKLM,Software\3Com\EL90xbc\CurrentVersion\NetRules,use,0,%SoftwareType%

;------------------------------------


[EL90x.Service.NT]
DisplayName     = %el90x.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\el90Xbc5.SYS
LoadOrderGroup  = NDIS
;AddReg         = TextModeFlags.reg.NT

;------------------------------------

[EL90x.EventLog.NT]
AddReg = el90x.AddEventLog.reg.NT

;------------------------------------

[EL90x.AddEventLog.reg.NT]
HKR,, EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\el90Xbc5.sys
HKR,, TypesSupported,   0x00010001, 7

;End Win 2k Exclusive----------------


[strings]
V_MS					="3Com"
V_3COM					="3Com"
Source_Disk_Name 			="ECD544P90X"	

ProviderName				="3Com Corporation"
el90x.Service.DispName 			="3Com 3C90X-BC Family PCI EtherLink Adapter"

ProductSoftwareDescription		="3Com 3C90X Adapter Driver"
ProductSoftwareTitle			="3Com 3C90x Adapter Driver"
ProductMajorVersion			="1"
ProductMinorVersion 			="0"
ProductSoftwareName			="EL90xbc"
ProductReview				="1"
SoftwareType				="driver"
NetRuleSoftwareType			="El90xbcSys ndisDriver El90xbcDriver"
NetRuleSoftwareBindForm			="""El90xbcSys"" yes no container"
NetRuleSoftwareClass			="El90xbcDriver basic"
NetRuleSoftwareBindable			="El90xbcDriver El90xAdapter non exclusive 100"

DISABLE					="Disable"
ENABLE					="Enable"
Enable_All_Caps				="ENABLE"
enum					="enum"
8021p 					="802.1p Support"
rx_checksum 				="Rx Checksum Offload"
tx_checksum 				="Tx Checksum Offload"

media_100_full 				="100 Mb, Full Duplex"
media_100_half				="100 Mb, Half Duplex"
media_10_full 				="10 Mb, Full Duplex"
media_10_half 				="10 Mb, Half Duplex"
media_100BaseFx_full			="100BASE-FX, Full Duplex"
media_100BaseFx_half			="100BASE-FX, Half Duplex"
media_10BaseFl_full			="10BASE-FL, Full Duplex"
media_10BaseFl_half			="10BASE-FL, Half Duplex"
media_10Base2 				="10BASE-2, Half Duplex"
media_10AUI				="AUI, Half Duplex"
media_type 				="Media Type"
media_default 				="HardwareDefault"
media_auto				="AutoSelect"
FLOW_CONTROL				="Flow Control"
hardware_default			="Hardware Default"

; Driver Information Entries
; These items will be set by IHV...
DriverMfgr="3Com"                                     	; IHV name
DriverVersionID="4.35.0.0"                            	; The IHV driver version
 BaseDriverFileName="El90xbc5.sys"               	; Key file for version
 BaseDriverFileVersion="4.35.0000.0"                   	; version of key file
; These items will be set by IHV and updated by OEM
DriverOEM="3Com"                                      	; name of the OEM
DriverFamily="NIC"                                   	; device family (NIC, Storage, Video...)
DriverProduct="NIC"                                   	; Specific Name of device (chipset, for example)
DriverDescription="Description - DriverInfo sample"     ; Description of device (product name, OS or system supported)
DriverOEMVersion="5.4.4.0"                          	; OEM-specified version

PCIEL9200LOM.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM1246103C.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM1247103C.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM1248103C.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM211914A4.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM303C1462.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM1101144D.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9200LOM802A1043.DeviceDesc=	"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM0013.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00E3.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00E4.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00C8.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00D4.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00D5.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00B8.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00B9.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM012A.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM012B.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM0122.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00F3.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM00F4.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOMC002.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOMC005.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
MOBILEEL9200LOM3500.DeviceDesc=		"3Com 3C920 Integrated Fast Ethernet Controller (3C905C-TX Compatible)"
PCIEL9055LOM.DeviceDesc=		"3Com 3C918 Integrated Fast Ethernet Controller (3C905B-TX Compatible)"
PCI\VEN_10b7&DEV_9058.DeviceDesc=	"3Com EtherLink 10/100 PCI Combo NIC (3C905B-COMBO)"
PCI\VEN_10b7&DEV_905A.DeviceDesc=	"3Com EtherLink 100 PCI Fiber NIC (3C905B-FX)"
PCI\VEN_10b7&DEV_9055.DeviceDesc=	"3Com EtherLink 10/100 PCI TX NIC (3C905B-TX)"
PCI\VEN_10b7&DEV_900A.DeviceDesc=	"3Com EtherLink PCI Fiber NIC (3C900B-FL)"
PCI\VEN_10b7&DEV_9004.DeviceDesc=	"3Com EtherLink PCI TPO NIC (3C900B-TPO)"
PCI\VEN_10b7&DEV_9005.DeviceDesc=	"3Com EtherLink PCI Combo NIC (3C900B-COMBO)"
PCI\VEN_10b7&DEV_9006.DeviceDesc=	"3Com EtherLink PCI TPC NIC (3C900B-TPC)"
PCI\VEN_10b7&DEV_9200&SUBSYS_100010B7.DeviceDesc=	"3Com EtherLink 10/100 PCI For Complete PC Management NIC (3C905C-TX)"
PCI\VEN_10b7&DEV_9200&SUBSYS_700010B7.DeviceDesc=	"3Com 10/100 Mini PCI Ethernet Adapter"
PCI\VEN_10b7&DEV_9201&SUBSYS_12B8103C.DeviceDesc=	"3Com 3C920B-EMB Integrated Fast Ethernet Controller"
PCI\VEN_10b7&DEV_9201&SUBSYS_233C1106.DeviceDesc=	"3Com 3C920B-EMB Integrated Fast Ethernet Controller"
PCI\VEN_10b7&DEV_9201&SUBSYS_B00F144D.DeviceDesc=	"3Com 3C920B-EMB Integrated Fast Ethernet Controller"
PCI\VEN_10b7&DEV_9201.DeviceDesc=			"3Com 3C920B-EMB Integrated Fast Ethernet Controller"
PCI\VEN_10b7&DEV_9202.DeviceDesc=			"3Com 3C920B-EMB-WNM Integrated Fast Ethernet Controller"
;------------------------------------

[DestinationDirs]
DefaultDestDir =11 
El90x.Driver.NT = 12
EL90x.ndis3.CopyFiles =12 
EL90x.ndis95.CopyFiles =11

;------------------------------------

[downPollRate]
HKR,,DownPollRate,,"8"
HKR,Ndi\params\DownPollRate,,,"8"
HKR,Ndi\params\DownPollRate,		ParamDesc,	, 	"Down Poll Rate"
HKR,Ndi\params\DownPollRate,		flag,			1,20,00,00,00
HKR,Ndi\params\DownPollRate,		optional,	, 	"0"
HKR,Ndi\params\DownPollRate,		type,		, 	%enum%
HKR,Ndi\params\DownPollRate\enum,	8,		,	 "8"
HKR,Ndi\params\DownPollRate\enum,	64,		,	 "64"

[downPollRate.NT]
HKR,,DownPollRate,,"8"
HKR,Ndi\params\DownPollRate,		ParamDesc,	, 	"Down Poll Rate"
HKR,Ndi\params\DownPollRate,		optional,	,	 "0"
HKR,Ndi\params\DownPollRate,		type,		,	 %enum%
HKR,Ndi\params\DownPollRate,          	default,        , 	"8"
HKR,Ndi\params\DownPollRate\enum,	8,		, 	"8"
HKR,Ndi\params\DownPollRate\enum,	64,		,	"64"

[FLOWCONTROL]
HKR,,FLOWCONTROL,,"ENABLE"
HKR,Ndi\params\FLOWCONTROL,		ParamDesc,	, 	%flow_control%
HKR,NDI\params\FLOWCONTROL,		flag,			1,30,00,00,00
HKR,Ndi\params\FLOWCONTROL,		type,		, 	%enum%
HKR,Ndi\params\FLOWCONTROL,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\FLOWCONTROL\enum,	ENABLE,		, 	%ENABLE%
HKR,Ndi\params\FLOWCONTROL\enum,	DISABLE,	, 	%DISABLE%

[FLOWCONTROL.NT]
HKR,,FLOWCONTROL,,"ENABLE"
HKR,Ndi\params\FLOWCONTROL,          	ParamDesc,      0, 	%flow_control%
HKR,Ndi\params\FLOWCONTROL,          	type,          	0, 	%enum%
HKR,Ndi\params\FLOWCONTROL,          	default,        0, 	%Enable_All_Caps%
HKR,Ndi\params\FLOWCONTROL\enum,      	ENABLE,        	0, 	%ENABLE%
HKR,Ndi\params\FLOWCONTROL\enum,      	DISABLE,       	0, 	%DISABLE%

[checksum]
HKR,Ndi\params\RxChecksum,		ParamDesc,	, 	%rx_checksum%
HKR,Ndi\params\RxChecksum,		type,		, 	%enum%
HKR,Ndi\params\RxChecksum,		default,	, 	"DISABLE"
HKR,Ndi\params\RxChecksum\enum,		ENABLE,		, 	%ENABLE%
HKR,Ndi\params\RxChecksum\enum,		DISABLE,	, 	%DISABLE%

HKR,Ndi\params\TxChecksum,		ParamDesc,	, 	%tx_checksum%
HKR,Ndi\params\TxChecksum,		type,	 	, 	%enum%
HKR,Ndi\params\TxChecksum,		default,	, 	"DISABLE"
HKR,Ndi\params\TxChecksum\enum,		ENABLE,		, 	%ENABLE%
HKR,Ndi\params\TxChecksum\enum,		DISABLE,	, 	%DISABLE%

[checksum.NT]
HKR,Ndi\params\RxChecksum,		ParamDesc,	, 	%rx_checksum%
HKR,Ndi\params\RxChecksum,		type,		, 	%enum%
HKR,Ndi\params\RxChecksum,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\RxChecksum\enum,		ENABLE,		, 	%ENABLE%
HKR,Ndi\params\RxChecksum\enum,		DISABLE,	, 	%DISABLE%

HKR,Ndi\params\TxChecksum,		ParamDesc,	, 	%tx_checksum%
HKR,Ndi\params\TxChecksum,		type,	 	, 	%enum%
HKR,Ndi\params\TxChecksum,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\TxChecksum\enum,		ENABLE,		, 	%ENABLE%
HKR,Ndi\params\TxChecksum\enum,		DISABLE,	, 	%DISABLE%

[8021psupport]
HKR,,8021psupport,,%DISABLE%
HKR,Ndi\params\8021psupport,		ParamDesc,	, 	%8021p%
HKR,NDI\params\8021psupport,		flag,			1,20,00,00,00
HKR,Ndi\params\8021psupport,		type,		, 	%enum%
HKR,NDI\params\8021psupport,		optional,	,	 "0"
HKR,Ndi\params\8021psupport\enum,	DISABLE,	, 	%DISABLE%
HKR,Ndi\params\8021psupport\enum,	ENABLE,		, 	%ENABLE%

[8021psupport.NT]
HKR,,8021psupport,,%DISABLE%
HKR,Ndi\params\8021psupport,		ParamDesc,	, 	%8021p%
HKR,Ndi\params\8021psupport,		type,		, 	%enum%
HKR,NDI\params\8021psupport,		optional,	,	 "0"
HKR,Ndi\params\8021psupport,		default,	, 	%DISABLE%
HKR,Ndi\params\8021psupport\enum,	DISABLE,	, 	%DISABLE%
HKR,Ndi\params\8021psupport\enum,	ENABLE,		,	%ENABLE%

[InitDelayCount]
HKR,,InitDelayCount,,"0"
HKR,Ndi\params\InitDelayCount,		ParamDesc,	, 	"InitDelayCount"
HKR,Ndi\params\InitDelayCount,		type,		, 	"int"
HKR,Ndi\Params\InitDelayCount,		min,        	, 	"0"
HKR,Ndi\Params\InitDelayCount,		max,        	, 	"60"
HKR,Ndi\Params\InitDelayCount,		step,       	, 	"1"
HKR,Ndi\Params\InitDelayCount,		Base,       	, 	"10"

[InitDelayCount.NT]
HKR,,InitDelayCount,,"0"
HKR,Ndi\params\InitDelayCount,		ParamDesc,	, 	"InitDelayCount"
HKR,Ndi\params\InitDelayCount,		type,		,	"int"
HKR,Ndi\params\InitDelayCount,		default,        , 	"0"
HKR,Ndi\Params\InitDelayCount,		min,        	, 	"0"
HKR,Ndi\Params\InitDelayCount,		max,        	, 	"60"
HKR,Ndi\Params\InitDelayCount,		step,       	, 	"1"
HKR,Ndi\Params\InitDelayCount,		Base,       	, 	"10"

[DoubleNego]
HKR,,DoubleNego,,%ENABLE%
HKR,Ndi\params\DoubleNego,		ParamDesc,	, 	"DoubleNego"
HKR,Ndi\params\DoubleNego,		type,		, 	%enum%
HKR,NDI\params\DoubleNego,		optional,	,	 "0"
HKR,Ndi\params\DoubleNego,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\DoubleNego\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\DoubleNego\enum,		ENABLE,		, 	%ENABLE%

[DoubleNego.NT]
HKR,,DoubleNego,,%ENABLE%
HKR,Ndi\params\DoubleNego,		ParamDesc,	, 	"DoubleNego"
HKR,Ndi\params\DoubleNego,		type,		, 	%enum%
HKR,NDI\params\DoubleNego,		optional,	,	 "0"
HKR,Ndi\params\DoubleNego,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\DoubleNego\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\DoubleNego\enum,		ENABLE,		,	%ENABLE%

[PHYCompat]
HKR,,PHYCompat,,%ENABLE%
HKR,Ndi\params\PHYCompat,		ParamDesc,	, 	"PHYCompat"
HKR,Ndi\params\PHYCompat,		type,		, 	%enum%
HKR,NDI\params\PHYCompat,		optional,	,	 "0"
HKR,Ndi\params\PHYCompat,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\PHYCompat\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\PHYCompat\enum,		ENABLE,		, 	%ENABLE%

[PHYCompat.NT]
HKR,,PHYCompat,,%ENABLE%
HKR,Ndi\params\PHYCompat,		ParamDesc,	, 	"PHYCompat"
HKR,Ndi\params\PHYCompat,		type,		, 	%enum%
HKR,NDI\params\PHYCompat,		optional,	,	 "0"
HKR,Ndi\params\PHYCompat,		default,	, 	%Enable_All_Caps%
HKR,Ndi\params\PHYCompat\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\PHYCompat\enum,		ENABLE,		,	%ENABLE%

[LnkChk]
HKR,,LnkChk,,%DISABLE%
HKR,Ndi\Params\LnkChk,          	ParamDesc,  	, 	"LnkChk"
HKR,Ndi\Params\LnkChk,          	type,       	, 	%enum%
HKR,Ndi\Params\LnkChk,          	optional,   	, 	"0"
HKR,Ndi\Params\LnkChk,          	default,   	, 	"DISABLE"
HKR,Ndi\params\LnkChk\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\LnkChk\enum,		ENABLE,		,	%ENABLE%

[LnkChk.NT]
HKR,,LnkChk,,%DISABLE%
HKR,Ndi\Params\LnkChk,          	ParamDesc,  	, 	"LnkChk"
HKR,Ndi\Params\LnkChk,          	type,       	, 	%enum%
HKR,Ndi\Params\LnkChk,          	optional,   	, 	"0"
HKR,Ndi\params\LnkChk,			default,	, 	"DISABLE"
HKR,Ndi\params\LnkChk\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\LnkChk\enum,		ENABLE,		,	%ENABLE%

[SWCblDet]
HKR,,SWCblDet,,"0"
HKR,Ndi\params\SWCblDet,,,"0"
HKR,Ndi\params\SWCblDet,		ParamDesc,	, 	"Software Cable Detect"
HKR,Ndi\params\SWCblDet,		optional,	, 	"0"
HKR,Ndi\params\SWCblDet,		type,		, 	%enum%
HKR,Ndi\params\SWCblDet,          	default,        , 	"Off"
HKR,Ndi\params\SWCblDet\enum,		0,		,	"Off"
HKR,Ndi\params\SWCblDet\enum,		1,		,	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		2,		,	"Enhanced"

[SWCblDet.NT]
HKR,,SWCblDet,,"0"
HKR,Ndi\Params\SWCblDet,          	ParamDesc,  	, 	"Software Cable Detect"
HKR,Ndi\Params\SWCblDet,          	type,       	, 	%enum%
HKR,Ndi\Params\SWCblDet,          	optional,   	, 	"0"
HKR,Ndi\params\SWCblDet,		default,	, 	"Off"
HKR,Ndi\params\SWCblDet\enum,		0,		, 	"Off"
HKR,Ndi\params\SWCblDet\enum,		1,		, 	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		2,		,	"Enhanced"

[SWCblDetMOBILE]
HKR,,SWCblDet,,"1"
HKR,Ndi\params\SWCblDet,,,"1"
HKR,Ndi\params\SWCblDet,		ParamDesc,	, 	"Software Cable Detect"
HKR,Ndi\params\SWCblDet,		optional,	, 	"0"
HKR,Ndi\params\SWCblDet,		type,		, 	%enum%
HKR,Ndi\params\SWCblDet,          	default,        , 	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		0,		,	"Off"
HKR,Ndi\params\SWCblDet\enum,		1,		,	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		2,		,	"Enhanced"

[SWCblDetMOBILE.NT]
HKR,,SWCblDet,,"1"
HKR,Ndi\Params\SWCblDet,          	ParamDesc,  	, 	"Software Cable Detect"
HKR,Ndi\Params\SWCblDet,          	type,       	, 	%enum%
HKR,Ndi\Params\SWCblDet,          	optional,   	, 	"0"
HKR,Ndi\params\SWCblDet,		default,	, 	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		0,		, 	"Off"
HKR,Ndi\params\SWCblDet\enum,		1,		, 	"Intermediate"
HKR,Ndi\params\SWCblDet\enum,		2,		,	"Enhanced"

[EnhLANPwrMgmt]
HKR,,EnhLANPwrMgmt,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,		ParamDesc,	, 	"Enh LAN Power Mgmt"
HKR,Ndi\params\EnhLANPwrMgmt,		optional,	, 	"0"
HKR,Ndi\params\EnhLANPwrMgmt,		type,		, 	%enum%
HKR,Ndi\params\EnhLANPwrMgmt,          	default,        , 	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	0,		,	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	1,		,	"On"

[EnhLANPwrMgmt.NT]
HKR,,EnhLANPwrMgmt,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,		ParamDesc,	, 	"Enh LAN Power Mgmt"
HKR,Ndi\params\EnhLANPwrMgmt,		optional,	, 	"0"
HKR,Ndi\params\EnhLANPwrMgmt,		type,		, 	%enum%
HKR,Ndi\params\EnhLANPwrMgmt,          	default,        , 	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	0,		,	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	1,		,	"On"

[EnhLANPwrMgmtMOBILE]
HKR,,EnhLANPwrMgmt,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,		ParamDesc,	, 	"Enh LAN Power Mgmt"
HKR,Ndi\params\EnhLANPwrMgmt,		optional,	, 	"0"
HKR,Ndi\params\EnhLANPwrMgmt,		type,		, 	%enum%
HKR,Ndi\params\EnhLANPwrMgmt,          	default,        , 	"On"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	0,		,	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	1,		,	"On"

[EnhLANPwrMgmtMOBILE.NT]
HKR,,EnhLANPwrMgmt,,"0"
HKR,Ndi\params\EnhLANPwrMgmt,		ParamDesc,	, 	"Enh LAN Power Mgmt"
HKR,Ndi\params\EnhLANPwrMgmt,		optional,	, 	"0"
HKR,Ndi\params\EnhLANPwrMgmt,		type,		, 	%enum%
HKR,Ndi\params\EnhLANPwrMgmt,          	default,        , 	"On"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	0,		,	"Off"
HKR,Ndi\params\EnhLANPwrMgmt\enum,	1,		,	"On"

[RWUMAGIC]
HKR,,RWUMAGIC,,%ENABLE%
HKR,Ndi\Params\RWUMAGIC,          	ParamDesc,  	, 	"RWU Magic Pkt"
HKR,Ndi\Params\RWUMAGIC,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUMAGIC,          	optional,   	, 	"0"
HKR,Ndi\params\RWUMAGIC,		default,	, 	"ENABLE"
HKR,Ndi\params\RWUMAGIC\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUMAGIC\enum,		ENABLE,		,	%ENABLE%

[RWUMAGIC.NT]
HKR,,RWUMAGIC,,%ENABLE%
HKR,Ndi\Params\RWUMAGIC,          	ParamDesc,  	, 	"RWU Magic Pkt"
HKR,Ndi\Params\RWUMAGIC,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUMAGIC,          	optional,   	, 	"0"
HKR,Ndi\params\RWUMAGIC,		default,	, 	"ENABLE"
HKR,Ndi\params\RWUMAGIC\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUMAGIC\enum,		ENABLE,		,	%ENABLE%

[RWUARP]
HKR,,RWUARP,,%DISABLE%
HKR,Ndi\Params\RWUARP,          	ParamDesc,  	, 	"RWU ARP"
HKR,Ndi\Params\RWUARP,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUARP,          	optional,   	, 	"0"
HKR,Ndi\params\RWUARP,			default,	, 	"DISABLE"
HKR,Ndi\params\RWUARP\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUARP\enum,		ENABLE,		,	%ENABLE%

[RWUARP.NT]
HKR,,RWUARP,,%DISABLE%
HKR,Ndi\Params\RWUARP,          	ParamDesc,  	, 	"RWU ARP"
HKR,Ndi\Params\RWUARP,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUARP,          	optional,   	, 	"0"
HKR,Ndi\params\RWUARP,			default,	, 	"DISABLE"
HKR,Ndi\params\RWUARP\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUARP\enum,		ENABLE,		,	%ENABLE%

[RWUPING]
HKR,,RWUPING,,%DISABLE%
HKR,Ndi\Params\RWUPING,          	ParamDesc,  	, 	"RWU Ping"
HKR,Ndi\Params\RWUPING,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUPING,          	optional,   	, 	"0"
HKR,Ndi\params\RWUPING,			default,	, 	"DISABLE"
HKR,Ndi\params\RWUPING\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUPING\enum,		ENABLE,		,	%ENABLE%

[RWUPING.NT]
HKR,,RWUPING,,%DISABLE%
HKR,Ndi\Params\RWUPING,          	ParamDesc,  	, 	"RWU Ping"
HKR,Ndi\Params\RWUPING,          	type,       	, 	%enum%
HKR,Ndi\Params\RWUPING,          	optional,   	, 	"0"
HKR,Ndi\params\RWUPING,			default,	, 	"DISABLE"
HKR,Ndi\params\RWUPING\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\RWUPING\enum,		ENABLE,		,	%ENABLE%

[STBYMAGIC]
HKR,,STBYMAGIC,,%ENABLE%
HKR,Ndi\Params\STBYMAGIC,          	ParamDesc,  	, 	"Stdby RWU Magic Pkt"
HKR,Ndi\Params\STBYMAGIC,          	type,       	, 	%enum%
HKR,Ndi\Params\STBYMAGIC,          	optional,   	, 	"0"
HKR,Ndi\params\STBYMAGIC,		default,	, 	"ENABLE"
HKR,Ndi\params\STBYMAGIC\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\STBYMAGIC\enum,		ENABLE,		,	%ENABLE%

[STBYMAGIC.NT]
HKR,,STBYMAGIC,,%ENABLE%
HKR,Ndi\Params\STBYMAGIC,          	ParamDesc,  	, 	"Stdby RWU Magic Pkt"
HKR,Ndi\Params\STBYMAGIC,          	type,       	, 	%enum%
HKR,Ndi\Params\STBYMAGIC,          	optional,   	, 	"0"
HKR,Ndi\params\STBYMAGIC,		default,	, 	"ENABLE"
HKR,Ndi\params\STBYMAGIC\enum,		DISABLE,	, 	%DISABLE%
HKR,Ndi\params\STBYMAGIC\enum,		ENABLE,		,	%ENABLE%

[STBYPATTERN]
HKR,,STBYPATTERN,,%ENABLE%
HKR,Ndi\Params\STBYPATTERN,          	ParamDesc,  	, 	"Stdby RWU Pattern"
HKR,Ndi\Params\STBYPATTERN,          	type,       	, 	%enum%
HKR,Ndi\Params\STBYPATTERN,          	optional,   	, 	"0"
HKR,Ndi\params\STBYPATTERN,		default,	, 	"ENABLE"
HKR,Ndi\params\STBYPATTERN\enum,	DISABLE,	, 	%DISABLE%
HKR,Ndi\params\STBYPATTERN\enum,	ENABLE,		,	%ENABLE%

[STBYPATTERN.NT]
HKR,,STBYPATTERN,,%ENABLE%
HKR,Ndi\Params\STBYPATTERN,          	ParamDesc,  	, 	"Stdby RWU Pattern"
HKR,Ndi\Params\STBYPATTERN,          	type,       	, 	%enum%
HKR,Ndi\Params\STBYPATTERN,          	optional,   	, 	"0"
HKR,Ndi\params\STBYPATTERN,		default,	, 	"ENABLE"
HKR,Ndi\params\STBYPATTERN\enum,	DISABLE,	, 	%DISABLE%
HKR,Ndi\params\STBYPATTERN\enum,	ENABLE,		,	%ENABLE%

; *****************************************************************************************
[EL90x.params.tx]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FULL,		0, 	%media_100_full%
HKR,Ndi\params\media_type\enum,		100HALF,		0, 	%media_100_half%
HKR,Ndi\params\media_type\enum,		10FULL,			0, 	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0, 	%media_10_half%

[EL90x.params.tx.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FULL,		0, 	%media_100_full%
HKR,Ndi\params\media_type\enum,		100HALF,		0, 	%media_100_half%
HKR,Ndi\params\media_type\enum,		10FULL,			0, 	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0, 	%media_10_half%

; *****************************************************************************************

[EL90x.params.tpo]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,,,%media_default%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%

[EL90x.params.tpo.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%

; *****************************************************************************************

[EL90x.params.tpc]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%

[EL90x.params.tpc.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%

; *****************************************************************************************
[EL90x.params.combo]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%
HKR,Ndi\params\media_type\enum,		10AUI,			0,	%media_10AUI%

[EL90x.params.combo.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%
HKR,Ndi\params\media_type\enum,		10AUI,			0,	%media_10AUI%

; *****************************************************************************************

[EL90x.params.CMBDLX]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FULL, 		0,	%media_100_full%
HKR,Ndi\params\media_type\enum,		100HALF,		0,	%media_100_half%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%
HKR,Ndi\params\media_type\enum,		10AUI,			0,	%media_10AUI%

[EL90x.params.CMBDLX.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FULL, 		0,	%media_100_full%
HKR,Ndi\params\media_type\enum,		100HALF,		0,	%media_100_half%
HKR,Ndi\params\media_type\enum,		10FULL, 		0,	%media_10_full%
HKR,Ndi\params\media_type\enum,		10HALF,			0,	%media_10_half%
HKR,Ndi\params\media_type\enum,		10BASE2,		0,	%media_10Base2%
HKR,Ndi\params\media_type\enum,		10AUI,			0,	%media_10AUI%

; *****************************************************************************************
[EL90x.params.fx]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FXFULL, 		0,	%media_100BaseFX_full%
HKR,Ndi\params\media_type\enum,		100FXHALF,		0,	%media_100BaseFX_half%

[EL90x.params.fx.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		100FXFULL, 		0,	%media_100BaseFX_full%
HKR,Ndi\params\media_type\enum,		100FXHALF,		0,	%media_100BaseFX_half%

; *****************************************************************************************

[EL90x.params.fl]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		flag,				1,20,00,00,00
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		Autoselect,		0, 	%media_auto%
HKR,Ndi\params\media_type\enum,		10FLFULL, 		0,	%media_10BaseFl_full%
HKR,Ndi\params\media_type\enum,		10FLHALF,		0,	%media_10BaseFl_half%

[EL90x.params.fl.NT]
HKR,,media_type,,%media_default%
HKR,Ndi\params\media_type,		default,		0,	%media_default%
HKR,Ndi\params\media_type,		ParamDesc,		0, 	%media_type%
HKR,Ndi\params\media_type,		type,			0, 	%enum%
HKR,Ndi\params\media_type,		optional,		0, 	"0"
HKR,Ndi\params\media_type\enum,		HardwareDefault,	0, 	%hardware_default%
HKR,Ndi\params\media_type\enum,		10FLFULL, 		0,	%media_10BaseFl_full%
HKR,Ndi\params\media_type\enum,		10FLHALF,		0,	%media_10BaseFl_half%



; *****************************************************************************************

[DriverInfoAddReg]
; This section is added to all INFs to add registry entries for Driver Info.
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileName,,%BaseDriverFileName%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%, BaseDriverFileVersion,,%BaseDriverFileVersion%


;(%VER w9x90xbc.INF - Installation file for 90x - v5.4.72)





