;
; SMC EZ Card 1000 (SMC9452TX V.2)
;
; (C)Copyright 1998-2003 SMC Networks, Inc.
; 
; All rights reserved
;
; INF File for NDIS5.1 Miniport Driver for Windows XP (x86) smc9452m.sys v6.14

[Version]
Signature	= "$windows nt$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %SMC%
CatalogFile	= smc9452m.CAT
DriverVer=05/15/2003, 6.14.0.0

[Manufacturer]
%SMC%	= SMC


[ControlFlags]

ExcludeFromSelect	= *

[SMC]
%SMC9452TXV2.DeviceDesc% = GeSingleLinkV2Copper.ndi, PCI\VEN_11AB&DEV_4320&SUBSYS_B45210B8





;-------------------------------------------------------------------------------
; Gigabit Ethernet Adapters <single link Version 2.0 Copper>

[GESingleLinkV2Copper.ndi]
AddReg		= smc9452m.reg, smc9452m.params, smc9452m.Copper.params, smc9452m.V2.Copper.params 
Characteristics	= 0x84
BusType		= 5
CopyFiles	= smc9452m.CopyFiles

[GESingleLinkV2Copper.ndi.Services]
AddService	= smc9452m, 2, smc9452m.Service, common.EventLog






;-------------------------------------------------------------------------------
; General Driver Parameters
;
[smc9452m.params]

HKR, Ndi\Params\NetworkAddress,	ParamDesc,,	%NetAddress%
HKR, Ndi\Params\NetworkAddress,	Type,,		"edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,,	"18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,,	"1"
HKR, Ndi\Params\NetworkAddress,	Default,,	""
HKR, Ndi\Params\NetworkAddress,	Optional,,	"1"

HKR, Ndi\Params\MaxFrameSize,	ParamDesc,,	%MaxFrSize%
HKR, Ndi\Params\MaxFrameSize,	Type,,		"int"
HKR, Ndi\Params\MaxFrameSize,	Base,,		"10"
HKR, Ndi\Params\MaxFrameSize,	Min,,		"12"
HKR, Ndi\Params\MaxFrameSize,	Max,,		"9014"
HKR, Ndi\Params\MaxFrameSize,	Step,,		"1"
HKR, Ndi\Params\MaxFrameSize,	Default,,	"1514"

HKR, Ndi\Params\HwChecksum,	ParamDesc,,	%HwCsum%
HKR, Ndi\Params\HwChecksum,	Type,,		"enum"
HKR, Ndi\Params\HwChecksum\enum,1,,		%On%
HKR, Ndi\Params\HwChecksum\enum,0,,		%Off%
HKR, Ndi\Params\HwChecksum,	Default,,	"1"

HKR, Ndi\Params\Moderate,	ParamDesc,,	%IntMod%
HKR, Ndi\Params\Moderate,	Type,,		"enum"
HKR, Ndi\Params\Moderate\enum,1,,		%On%
HKR, Ndi\Params\Moderate\enum,0,,		%Off%
HKR, Ndi\Params\Moderate,	Default,,	"1"

HKR, Ndi\Params\FixedIntMod,	ParamDesc,,	%MaxIrq%
HKR, Ndi\Params\FixedIntMod,	Type,,		"int"
HKR, Ndi\Params\FixedIntMod,	Base,,		"10"
HKR, Ndi\Params\FixedIntMod,	Min,,		"1000"
HKR, Ndi\Params\FixedIntMod,	Max,,		"30000"
HKR, Ndi\Params\FixedIntMod,	Step,,		"1"
HKR, Ndi\Params\FixedIntMod,	Default,,	"5000"

HKR, Ndi\Params\MessageLog,	ParamDesc,,	%LogMsg%
HKR, Ndi\Params\MessageLog,	Type,,		"enum"
HKR, Ndi\Params\MessageLog\enum,4,,		%Non%
HKR, Ndi\Params\MessageLog\enum,3,,		%Err%
HKR, Ndi\Params\MessageLog\enum,2,,		%Wrn%
HKR, Ndi\Params\MessageLog\enum,1,,		%Sta%
HKR, Ndi\Params\MessageLog\enum,0,,		%All%
HKR, Ndi\Params\MessageLog,	Default,,	"1"

HKR, Ndi\Params\MaxReceives,	ParamDesc,,	%NumRcv%
HKR, Ndi\Params\MaxReceives,	Type,,		"int"
HKR, Ndi\Params\MaxReceives,	Base,,		"10"
HKR, Ndi\Params\MaxReceives,	Min,,		"3"
HKR, Ndi\Params\MaxReceives,	Max,,		"500"
HKR, Ndi\Params\MaxReceives,	Step,,		"1"
HKR, Ndi\Params\MaxReceives,	Default,,	"50"

HKR, Ndi\Params\MaxTransmits,	ParamDesc,,	%NumTx%
HKR, Ndi\Params\MaxTransmits,	Type,,		"int"
HKR, Ndi\Params\MaxTransmits,	Base,,		"10"
HKR, Ndi\Params\MaxTransmits,	Min,,		"4"
HKR, Ndi\Params\MaxTransmits,	Max,,		"200"
HKR, Ndi\Params\MaxTransmits,	Step,,		"1"
HKR, Ndi\Params\MaxTransmits,	Default,,	"50"

HKR, Ndi\Params\AutoNegotiation_A,	ParamDesc,,	%AutonegA%
HKR, Ndi\Params\AutoNegotiation_A,	Type,,		"enum"
HKR, Ndi\Params\AutoNegotiation_A\enum,2,,		%Sense%
HKR, Ndi\Params\AutoNegotiation_A\enum,1,,		%On%
HKR, Ndi\Params\AutoNegotiation_A\enum,0,,		%Off%
HKR, Ndi\Params\AutoNegotiation_A,	Default,,	"1"

HKR, Ndi\Params\DuplexCapabilities_A,	ParamDesc,,	%DupCapA%
HKR, Ndi\Params\DuplexCapabilities_A,	Type,,		"enum"
HKR, Ndi\Params\DuplexCapabilities_A\enum,3,,		%both%
HKR, Ndi\Params\DuplexCapabilities_A\enum,2,,		%full%
HKR, Ndi\Params\DuplexCapabilities_A\enum,1,,		%half%
HKR, Ndi\Params\DuplexCapabilities_A,	Default,,	"3"

HKR, Ndi\Params\FlowControl_A,	ParamDesc,,	%FlowCtrlA%
HKR, Ndi\Params\FlowControl_A,	Type,,		"enum"
HKR, Ndi\Params\FlowControl_A\enum,3,,		%bothFC%
HKR, Ndi\Params\FlowControl_A\enum,2,,		%sym%
HKR, Ndi\Params\FlowControl_A\enum,1,,		%asym%
HKR, Ndi\Params\FlowControl_A\enum,0,,		%noFc%
HKR, Ndi\Params\FlowControl_A,	Default,,	"3"

HKR,, MaxMulticast,,         "128"
HKR,, WaitForRxResources,,   "1"
HKR,, SGMapRegistersNeeded,, "64"


;-------------------------------------------------------------------------------
; Additional Driver Parameters for Single Link Copper Adapters
;
 [smc9452m.Copper.params]
;
; Configurable Parameters
;
HKR, Ndi\Params\Role_A,	ParamDesc,,	%RoleA%
HKR, Ndi\Params\Role_A,	Type,,		"enum"
HKR, Ndi\Params\Role_A\enum,3,,		%Slave%
HKR, Ndi\Params\Role_A\enum,2,,		%Master%
HKR, Ndi\Params\Role_A\enum,0,,		%Auto%
HKR, Ndi\Params\Role_A,	Default,,	"0"


;-------------------------------------------------------------------------------
; Additional Driver Parameters for Version 2.0 Copper Adapters
;
[smc9452m.V2.Copper.params]
;
; Configurable Parameters
;

HKR, Ndi\Params\WakeUpModeCap_A,       ParamDesc,,	%WakeUpCaps%
HKR, Ndi\Params\WakeUpModeCap_A,       type,,		"enum"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  0,,		"None"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  15,,		"OS Controlled"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  25,,		"Magic Packet"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  26,,		"Pattern Match"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  27,,		"Magic Packet and Pattern Match"
HKR, Ndi\Params\WakeUpModeCap_A\enum,  28,,		"Link Change"
HKR, Ndi\Params\WakeUpModeCap_A, Default,,		"15"

HKR, Ndi\Params\Speed_A,       ParamDesc,,	%Speed%
HKR, Ndi\Params\Speed_A,       type,,		"enum"
HKR, Ndi\Params\Speed_A\enum,  1,,		"Auto"
HKR, Ndi\Params\Speed_A\enum,  2,,		"10"
HKR, Ndi\Params\Speed_A\enum,  3,,		"100"
HKR, Ndi\Params\Speed_A\enum,  4,,		"1000"
HKR, Ndi\Params\Speed_A,	Default,,	"1"

HKR,, WaitForRxResources,,   "0"




;-------------------------------------------------------------------------------
; General Registry Entries
;
[smc9452m.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi\Interfaces, UpperRange,, "ndis5"
HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "smc9452m"

[smc9452m.Service]
DisplayName	= %smc9452m.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\smc9452m.sys
LoadOrderGroup = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\smc9452m.sys"
HKR,, TypesSupported,	0x00010001, 7

;-------------------------------------------------------------------------------
; Source Files
;
[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
smc9452m.sys	= 1,,

[smc9452m.CopyFiles]
smc9452m.sys,,,2


;-------------------------------------------------------------------------------
; Destination Directories
;
[DestinationDirs]

DefaultDestDir = 11
smc9452m.CopyFiles	= 12

;-------------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
SMC = "SMC"
NetAddress              = "Network Address"
MaxFrSize               = "Maximum Frame Size"
HwCsum                  = "Hardware Checksumming"
WakeUpCaps              = "Wake Up Capabilities"
Speed	                = "LinkSpeed"
IntMod                  = "Interrupt Moderation"
MaxIrq                  = "Max IRQ per Sec"
LogMsg                  = "Log Status Messages"
NumRcv                  = "Number of Receive Buffers"
NumTx                   = "Number of Transmit Buffers"
RLMT                    = "RLMT Mode"
Link                    = "CLS"             
OtherPort               = "CLP"                  
Segment                 = "CLPSS" 
Preferred               = "Preferred Port"
Sense			= "Auto-Sense"
On                      = "On"
Off                     = "Off"
Non                     = "None"
Err                     = "Errors"
Wrn                     = "Warnings"
Sta                     = "Status Messages"
All                     = "All Messages"
A                       = "A"
B                       = "B"
AutonegA		= "Autonegotiation Port A"
AutonegB		= "Autonegotiation Port B"
DupCapA			= "DuplexCapabilities Port A"
DupCapB			= "DuplexCapabilities Port B"
RoleA			= "Role on Port A"
RoleB			= "Role on Port B"
Slave			= "Slave"
Master			= "Master"
Auto			= "Auto"
both			= "Half and Full Duplex"
full			= "Full Duplex"
half			= "Half Duplex"
FlowCtrlA		= "FlowControl Port A"
FlowCtrlB		= "FlowControl Port B"
bothFC			= "Asymmetrical and Symmetrical Flow Control"
sym			= "Symmetrical Flow Control"
asym			= "Asymmetrical Flow Control"
noFc			= "No Flow Control"

SMC9452TXV2.DeviceDesc = "SMC EZ Card 1000 (SMC9452TX V.2)"



smc9452m.DriverDesc	= "NDIS5.1 Miniport Driver for SMC EZ Card 1000 (SMC9452TX V.2)"

DriverDisk		= "SMC EZ Card 1000 (SMC9452TX V.2) Installation Disk"

HelpText		= "This SMC network adapter connects you to the network."


