;***********************************************************************
;
; WLAN.INF
;
;   This installation script supports Windows 95, 98, Me, 2000 & XP
;   for the 802.11b Wireless LAN Adapters.
;
;   Copyright (c) 2001, 2002
;   All Rights Reserved.
;
;***********************************************************************

[Version]
 DriverVer           = 01/17/2003, 3.0.2
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
; CatalogFile         = Smc2662w32m.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = *

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]

 %USB_DESC_STR%     = WLAN_USB,         USB\VID_09AA&PID_3642
 %USB_DESC_STR%     = WLAN_USB,         USB\VID_0707&PID_EE04

;===============
; WLAN USB Card
;===============
[WLAN_USB]
 AddReg    = WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles = WLAN_DRIVER_USB, WLAN_CONFIG

[WLAN_USB.ME]
 AddReg    = WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles = WLAN_DRIVER_USB, WLAN_CONFIG

[WLAN_USB.NT]
 AddReg    = WLAN_USB.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles = WLAN_DRIVER_USB.NT
 BusType   = 0
 Characteristics= 0x84

[WLAN_USB.NT.Services]
 AddService= "PRISM_USB", 2, WLAN_DRIVER_USB.Service, WLAN_DRIVER.EventLog

[WLAN_USB.NT.CoInstallers]
 AddReg    = WLAN_COINSTALL.reg.NT

[WLAN_USB.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_09AA&PID_3642"
 HKR,,PlatformId,0,"0"
 HKR,,VendorDesc,0,%USB_DESC_STR%
 HKR,,LoadFirmware,0,1
 HKR,NDI\params\LoadFirmware,,0,1

;###############################################################################
[WLAN_COINSTALL.reg.NT]
 HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMCFG.cpl,NdiProc"

[WLAN_DRIVER.Service]
 DisplayName    = %WLAN_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\WLANNDS.sys
 LoadOrderGroup = NDIS

[WLAN_DRIVER_USB.Service]
 DisplayName    = %WLAN_SERVICE_DISPLAY_USB%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\SMCWUSB.sys
 LoadOrderGroup = NDIS

[WLAN_DRIVER.EventLog]
 AddReg         = WLAN_DRIVER.EventLog.reg

[WLAN_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_USB.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_USB"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"SMCWUSB.sys"

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
; HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,Configure"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,NDI\params\ListenInterval,,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,0,1

 HKR,defaults,RTSThresh,0,2432
 HKR,NDI\params\RTSThresh,,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,defaults,FragThresh,0,2432
 HKR,NDI\params\FragThresh,,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,defaults,PreambleMode,0,1
 HKR,NDI\params\PreambleMode,,0,1
 HKR,Ndi\params\PreambleMode,default,0,1
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,1

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,1

 HKR,defaults,AdhocDemoMode,0,0
 HKR,NDI\params\AdhocDemoMode,,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,0
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,enum
 HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,0,1

 HKR,defaults,LoadFirmware,0,1
;HKR,NDI\params\LoadFirmware,,0,1 ; Moved to device specific entry
 HKR,Ndi\params\LoadFirmware,default,0,1
 HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
 HKR,NDI\params\LoadFirmware,type,,enum
 HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
 HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
 HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
 HKR,NDI\params\LoadFirmware,optional,0,1

 HKR,defaults,PDwellTime,0,120
 HKR,NDI\params\PDwellTime,,0,120
 HKR,Ndi\params\PDwellTime,default,0,120
 HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
 HKR,NDI\params\PDwellTime,type,0,int
 HKR,NDI\params\PDwellTime,flag,1,20,00,00,00
 HKR,NDI\params\PDwellTime,min,0,0
 HKR,NDI\params\PDwellTime,max,0,1000
 HKR,NDI\params\PDwellTime,step,0,10
 HKR,NDI\params\PDwellTime,optional,0,1

 HKR,defaults,11dMode,0,0
 HKR,NDI\params\11dMode,,0,0
 HKR,Ndi\params\11dMode,default,0,0
 HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
 HKR,NDI\params\11dMode,type,,enum
 HKR,NDI\params\11dMode,flag,1,30,00,00,00
 HKR,NDI\params\11dMode\enum,0,,"None"
 HKR,NDI\params\11dMode\enum,1,,"Strict"
 HKR,NDI\params\11dMode\enum,2,,"Flexible"
 HKR,NDI\params\11dMode,optional,0,1

;###############################################################################
[DestinationDirs]
CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 WLAN_DRIVER            = 11 ; Win9x=%windir%\system
 WLAN_DRIVER_USB        = 11 ; Win9x=%windir%\system
 WLAN_CONFIG            = 11 ; Win9x=%windir%\system
 WLAN_DRIVER.NT         = 12 ; Win2k=%windir%\system32\drivers
 WLAN_DRIVER_USB.NT     = 12 ; Win2k=%windir%\system32\drivers

[WLAN_CONFIG]
 PRISMCFG.dll           ; Win9x NDI
 PRISMRES.dll
 PRISMIOC.dll

[WLAN_DRIVER]
 WLANNDS.sys

[WLAN_DRIVER_USB]
 SMCWUSB.sys

[WLAN_DRIVER.NT]
 WLANNDS.sys
 PRISMRES.dll
 PRISMIOC.dll
 PRISMCFG.CPL

[WLAN_DRIVER_USB.NT]
 SMCWUSB.sys
 PRISMRES.dll
 PRISMIOC.dll
 PRISMCFG.CPL

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMCFG.dll           = 1
 SMCWUSB.sys        = 1
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1

[SourceDisksFiles.ME]   ; WinMe
 PRISMCFG.dll           = 1
 SMCWUSB.sys        = 1
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 SMCWUSB.sys        = 1
 PRISMRES.dll           = 1
 PRISMIOC.dll           = 1
 PRISMCFG.cpl           = 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = " "
 VER_VENDOR_NAME_STR    = " "

 WLAN_SERVICE_DISPLAY  = "Wireless LAN Driver"
 WLAN_SERVICE_DISPLAY_USB  = "Wireless LAN USB Driver"
 INSTALL_DISK_STR       = "Wireless LAN Install Disk"

 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"
 LOAD_FIRMWARE_STR      = "Firmware Download"
 PDWELL_STR             = "Passive Scan Dwell Time"
 MDC_CONTROL_STR        = "802.11D Control"

 USB_DESC_STR           = "SMCWUSB32 802.11b Wireless LAN USB Card"

