;***********************************************************************
; PRISMA02.INF
;
;   This installation script supports Windows 98, Me, 2000 and XP for the
;   PRISM 802.11a/g Adapters.
;
;   Copyright 2001-2004
;***********************************************************************

[Version]
 DriverVer = 12/05/2003, 1.00.6.0
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
;CatalogFile         = PRISMA02.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = VID_2001&PID_3761

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %A021_DESC_STR%     = PRISM_A021,        USB\VID_2001&PID_3761

;==========
[PRISM_A021]       ; Win9x
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_A021.ME]    ; WinMe
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_A021.NT]    ; Win2k
 AddReg         = PRISM_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 0
 Characteristics= 0x84

[PRISM_A021.NT.Services]
 AddService= "PRISM_A02", 2, PRISM_DRIVER_A02.Service, PRISM_DRIVER.EventLog

[PRISM_A021.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_A021.reg]
 HKR,Ndi,DeviceID,0,"USB\VID_2001&PID_3761"
; 0x3890 = 14480
 HKR,,PlatformID,0,14480
 HKR,,VendorDesc,0,%A021_DESC_STR%

;###############################################################################
[PRISM_COINSTALL.reg.NT]
; HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMNDI.dll,NdiProc"

[PRISM_DRIVER_A02.Service]
 DisplayName    = %A02_SERVICE_STR%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMA02.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################

[COMMON_A02_DEL.reg]
 HKR,                   ,FWFileName

[COMMON_A02.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_A02"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMA02.sys"
;HKR,                   ,CardBusBridgeLatencyTimer  ,0  ,"32"
;HKR,                   ,CardBusBridgeCacheLineSize ,0  ,"8"

[COMMON_NDIS.reg]
; Win9X
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM_A02"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 ;HKR,NDI                ,NdiInstaller           ,0      ,"PRISMNDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM_A02"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
 ;HKR,                   ,EnumPropPages32        ,0      ,"PRISMNDI.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,NDI\params\RTSThresh,,0,2347
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,step,0,1
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,NDI\params\FragThresh,,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,NDI\params\ShortRetryLimit,,0,7
 HKR,NDI\params\ShortRetryLimit,default,0,7
 HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
 HKR,NDI\params\ShortRetryLimit,type,,int
 HKR,NDI\params\ShortRetryLimit,min,0,1
 HKR,NDI\params\ShortRetryLimit,max,0,255
 HKR,NDI\params\ShortRetryLimit,step,0,1
 HKR,NDI\params\ShortRetryLimit,optional,0,1

 HKR,NDI\params\LongRetryLimit,,0,4
 HKR,NDI\params\LongRetryLimit,default,0,4
 HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
 HKR,NDI\params\LongRetryLimit,type,0,int
 HKR,NDI\params\LongRetryLimit,min,0,1
 HKR,NDI\params\LongRetryLimit,max,0,255
 HKR,NDI\params\LongRetryLimit,step,0,1
 HKR,NDI\params\LongRetryLimit,optional,0,1

 HKR,,ConfigProfile,0,256
 HKR,NDI\params\ConfigProfile,,0,256
 HKR,NDI\params\ConfigProfile,default,0,256
 HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
 HKR,NDI\params\ConfigProfile,type,,enum
 HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
 HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
 HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
 HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
 HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
 HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
 HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
 HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
 HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
 HKR,NDI\params\ConfigProfile,optional,0,1

 HKR,,NitroMode,0,"1"
 HKR,NDI\params\NitroMode,,0,1
 HKR,NDI\params\NitroMode,default,0,1
 HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
 HKR,NDI\params\NitroMode,type,,enum
 HKR,NDI\params\NitroMode,flag,1,30,00,00,00
 HKR,NDI\params\NitroMode\enum,0,,%OFF_STR%
 HKR,NDI\params\NitroMode\enum,1,,%ON_STR%
 HKR,NDI\params\NitroMode,optional,0,1

 HKR,,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
 HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
 HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
 HKR,NDI\params\PSMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]
; PRISMNDI.dll
; PRISMAPI.dll
; PRISMSVR.exe

[PRISM_NDI.copy.ME]
; PRISMNDI.dll
; PRISMAPI.dll
; PRISMSVR.exe

[PRISM_COINSTALL.copy.NT]
; PRISMNDI.dll           ; Win2k CoInstaller
; PRISMAPI.dll
; PRISMSVR.exe

[PRISM_DRIVER.copy]
 PRISMA02.sys
; PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
 PRISMA02.sys
; PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
 PRISMA02.sys

[PRISM_APPLET.copy]

[PRISM_APPLET.copy.ME]

[PRISM_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 PRISMA02.sys           = 1
; PRISMIOC.vxd           = 1,win9x
; PRISMNDI.dll           = 1,win9x
; PRISMAPI.dll           = 1
; PRISMSVR.exe           = 1

[SourceDisksFiles.ME]   ; WinMe
 PRISMA02.sys           = 1
; PRISMIOC.vxd           = 1,win9x
; PRISMNDI.dll           = 1,win9x
; PRISMAPI.dll           = 1
; PRISMSVR.exe           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
 PRISMA02.sys           = 1
; PRISMNDI.dll           = 1,win2k
; PRISMAPI.dll           = 1
; PRISMSVR.exe           = 1

;###############################################################################
[Strings]
;String ID               = String Text
;---------                 -----------
 VER_VENDOR_STR          = ""
 VER_VENDOR_NAME_STR     = ""
 INSTALL_DISK_STR        = "Wireless LAN Install Disk"

 A021_DESC_STR           = "IEEE 802.11g USB2.0 Wireless Network Adapter-PN"
 A02_SERVICE_STR         = "IEEE802.11g Wireless USB2.0 Driver"

 ON_STR                  = "On"
 OFF_STR                 = "Off"
 RTSTHRESH_STR           = "RTS Threshold"
 FRAGTHRESH_STR          = "Fragmentation Threshold"
 AUTHENT_TYPE_STR        = "Authentication Algorithm"
 POWER_SAVE_STR          = "Power Save Mode"
 POWER_SAVE_OFF_STR      = "Disabled"
 POWER_SAVE_DYN_STR      = "Dynamic"
 POWER_SAVE_MAX_STR      = "Maximum"
 SHORT_RETRY_STR         = "Short Retry Limit"
 LONG_RETRY_STR          = "Long Retry Limit"
 CONFIG_PROFILE          = "Configuration Profile"
 CONFIG_PROF_B_ONLY      = "B only"
 CONFIG_PROF_MIXED       = "Mixed"
 CONFIG_PROF_MIXED_LONG  = "Mixed Long"
 CONFIG_PROF_G_ONLY      = "G only"
 CONFIG_PROF_TEST        = "Test"
 CONFIG_PROF_B_WIFI      = "B WiFi"
 CONFIG_PROF_MIXED_SHORT = "Mixed Short"
 CONFIG_PROF_WIFI_SPEC   = "WiFi Spec"
 NITRO_MODE              = "Nitro Mode"

