;USR-ACTNNIC.inf
;***********************************************************************
;
; BELNIC.INF
;
;   This installation script supports Windows 98,Me,2000 & XP for the
;   Belkin 11Mbps Wireless LAN Adapters.
;
;   Copyright (c) 2002 Belkin Components
;   All Rights Reserved.
;   Developed by Belkin Components. -- http://www.belkin.com
;
;***********************************************************************

[Version]
 DriverVer = 03/13/2002, 1.31.0313.2002
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
;CatalogFile         = BELNIC.cat
;MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = PCMCIA\Belkin-11Mbps_Wireless_Notebook_Network_Adapter-3D8C
 ExcludeFromSelect   = PCI\VEN_1638&DEV_1100&SUBSYS_11001638
 ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_06011799

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList,NTx86.5.1

[DeviceList]
 %PRISM_PCMCIA1_STR% = PRISM_PCMCIA1, PCMCIA\Belkin-11Mbps_Wireless_Notebook_Network_Adapter-3D8C
 %PRISM_PCI1_STR%    = PRISM_PCI1,    PCI\VEN_1638&DEV_1100&SUBSYS_11001638
 %PRISM_PCI2_STR%    = PRISM_PCI2,    PCI\VEN_1260&DEV_3873&SUBSYS_06011799

[DeviceList.NTx86.5.1]
 %PRISM_PCMCIA1_STR% = PRISM_PCMCIA1_XP, PCMCIA\Belkin-11Mbps_Wireless_Notebook_Network_Adapter-3D8C
 %PRISM_PCI1_STR%    = PRISM_PCI1_XP,    PCI\VEN_1638&DEV_1100&SUBSYS_11001638
 %PRISM_PCI2_STR%    = PRISM_PCI2_XP,    PCI\VEN_1260&DEV_3873&SUBSYS_06011799

;==========================================
[PRISM_PCMCIA1]         ; Win9x
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg

[PRISM_PCMCIA1.NT]      ; Win2k
 AddReg         = PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 8     ; PCMCIA
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCMCIA1.NT.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCMCIA1.NT.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCMCIA1.reg]
 HKR,Ndi        ,DeviceID,0,"PCMCIA\Belkin-11Mbps_Wireless_Notebook_Network_Adapter-3D8C"

;==========================================
[PRISM_PCI1]            ; Win9x
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 

[PRISM_PCI1.NT]         ; Win2k
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI1.NT.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI1.NT.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCI1.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"

;==========================================
[PRISM_PCI2]            ; Win9x
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 

[PRISM_PCI2.NT]         ; Win2k
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI2.NT.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI2.NT.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCI2.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"

;==========================================
[PRISM_PCMCIA1_XP]      ; WinXP
 AddReg         = PRISM_PCMCIA1_XP.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 8     ; PCMCIA
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCMCIA1_XP.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCMCIA1_XP.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.XP

[PRISM_PCMCIA1_XP.reg]
 HKR,Ndi        ,DeviceID,0,"PCMCIA\Belkin-11Mbps_Wireless_Notebook_Network_Adapter-3D8C"

;==========================================
[PRISM_PCI1_XP]         ; WinXP
 AddReg         = PRISM_PCI1_XP.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI1_XP.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI1_XP.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.XP

[PRISM_PCI1_XP.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"

;==========================================
[PRISM_PCI2_XP]         ; WinXP
 AddReg         = PRISM_PCI2_XP.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI2_XP.Services]
 AddService     = "BEL", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI2_XP.CoInstallers]
 
 AddReg         = PRISM_COINSTALL.reg.XP

[PRISM_PCI2_XP.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"

;###############################################################################

[PRISM_COINSTALL.reg.NT]
 HKR,           ,CoInstallers32         ,0x00010000     ,"BELCFG.cpl,NdiProc"

[PRISM_COINSTALL.reg.XP]
 HKR,           ,CoInstallers32         ,0x00010000     ,"BELCFG.cpl,NdiProc"

[PRISM_DRIVER.Service]
 DisplayName    = %PRISM_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\BELNDS.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_PCMCIA.reg]
;RegKey,SubKey          ,Name                   ,Type   ,Value
;-------------          -----                   -----   ------
 HKR,NDI                ,Service                ,0      ,"BEL"
 HKR,NDI                ,CardType               ,0      ,"PCMCIA"
 HKR,                   ,BusType                ,0      ,"8"
 HKR,                   ,DeviceVxDs             ,0      ,"BELNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_PCI.reg]
 HKR,NDI                ,Service                ,0      ,"BEL"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"BELNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"BELCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"BEL"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"BELCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON.reg]
 HKR,                   ,BELIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,0,1

 HKR,defaults,RTSThresh,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,defaults,FragThresh,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,defaults,PreambleMode,0,1
 HKR,Ndi\params\PreambleMode,default,0,1
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,1

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,1

 HKR,defaults,AdhocDemoMode,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,0
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,enum
 HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,0,1

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "Belkin"
 VER_VENDOR_NAME_STR    = "Belkin Components"

 PRISM_PCMCIA1_STR      = "Belkin 11Mbps Wireless Notebook Network Adapter"
 PRISM_PCI1_STR         = "Belkin 11Mbps Wireless PCI Adapter Card"
 PRISM_PCI2_STR         = "Belkin 11Mbps Wireless Desktop PCI Adapter Card"

 PRISM_SERVICE_DISPLAY  = "Belkin 11Mbps Wireless LAN Driver"
 INSTALL_DISK_STR       = "Belkin 11Mbps Wireless LAN Install Disk"

 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"

