;***********************************************************************
;
; PRISMNIC.INF
;
;
;***********************************************************************

[Version]
 DriverVer = 01/17/2002, 1.7.37
 Signature           = "$Chicago$"
 Compatible          = 1
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318}
 Provider            = %VER_VENDOR_STR%
;CatalogFile         = PRISMNIC.cat
 MillenniumPreferred = .ME

[ControlFlags]
;Exclude all PNP adapters from user selection
 ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_35011186
 ExcludeFromSelect   = PCI\VEN_1260&DEV_3873&SUBSYS_38731260
 ExcludeFromSelect   = USB\VID_2474&PID_3642
 ExcludeFromSelect   = USB\VID_09AA&PID_3642

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %PRISM_PCI1_STR%    = PRISM_PCI1,    PCI\VEN_1260&DEV_3873&SUBSYS_35011186
 %PRISM_PCI2_STR%    = PRISM_PCI2,    PCI\VEN_1260&DEV_3873&SUBSYS_38731260
 %PRISM_USB1_STR%    = PRISM_USB1,    USB\VID_2474&PID_3642
 %PRISM_USB1_STR%    = PRISM_USB1,    USB\VID_09AA&PID_3642

;==========================================
[PRISM_PCI1]            ; Win9x
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_PCI1.ME]         ; WinMe
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCI1.ME.ME]      ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCI1.NT]         ; Win2k
 AddReg         = PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI1.NT.Services]
 AddService     = "PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI1.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCI1.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_35011186"

;==========================================
[PRISM_PCI2]            ; Win9x
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_PCI2.ME]         ; WinMe
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCI2.ME.ME]      ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_PCI2.NT]         ; Win2k
 AddReg         = PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 5     ; PCI
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_PCI2.NT.Services]
 AddService     = "PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_PCI2.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_PCI2.reg]
 HKR,Ndi        ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_38731260"

;==========================================
[PRISM_USB1]            ; Win9x
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy

[PRISM_USB1.ME]         ; WinMe
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_USB1.ME.ME]      ; WinMe - Same as .ME (Needed for Update Driver)
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME

[PRISM_USB1.NT]         ; Win2k
 AddReg         = PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles      = PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
 BusType        = 0     ; USB
 Characteristics= 0x84  ; NCF_PHYSICAL | NCF_HAS_UI

[PRISM_USB1.NT.Services]
 AddService     = "PRISM_USB", 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog

[PRISM_USB1.NT.CoInstallers]
 CopyFiles      = PRISM_COINSTALL.copy.NT
 AddReg         = PRISM_COINSTALL.reg.NT

[PRISM_USB1.reg]
 HKR,Ndi        ,DeviceID,0,"USB\VID_2474&PID_3642"

;###############################################################################

[PRISM_COINSTALL.reg.NT]
 HKR,           ,CoInstallers32         ,0x00010000     ,"PRISMCFG.cpl,NdiProc"

[PRISM_DRIVER.Service]
 DisplayName    = %PRISM_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMNDS.sys
 LoadOrderGroup = NDIS

[PRISM_USB_DRIVER.Service]
 DisplayName    = %PRISM_USB_SERVICE_DISPLAY%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\PRISMUSB.sys
 LoadOrderGroup = NDIS

[PRISM_DRIVER.EventLog]
 AddReg         = PRISM_DRIVER.EventLog.reg

[PRISM_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

;###############################################################################
[COMMON_PCMCIA.reg]
;RegKey,SubKey          ,Name                   ,Type   ,Value
;-------------          -----                   -----   ------
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCMCIA"
 HKR,                   ,BusType                ,0      ,"8"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_PCI.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM"
 HKR,NDI                ,CardType               ,0      ,"PCI"
 HKR,                   ,BusType                ,0      ,"5"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMNDS.sys"
 HKR,                   ,EnableIRQSharing       ,1      ,01,00,00,00
 HKR,                   ,IOBaseAddress          ,1      ,02,00,00,00
 HKR,                   ,InterruptNumber        ,1      ,04,00,00,00

[COMMON_USB.reg]
 HKR,NDI                ,Service                ,0      ,"PRISM_USB"
 HKR,NDI                ,CardType               ,0      ,"USB"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"PRISMUSB.sys"

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
 HKR,NDI                ,NdiInstaller           ,0      ,"PRISMCFG.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"PRISM"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON_NDIS.reg.NT]
 HKR,                   ,EnumPropPages32        ,0      ,"PRISMCFG.cpl,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

 HKR,defaults,PSMode,0,1
 HKR,NDI\params\PSMode,,0,1
 HKR,Ndi\params\PSMode,default,0,1
 HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
 HKR,NDI\params\PSMode,type,,enum
 HKR,NDI\params\PSMode,flag,1,30,00,00,00
 HKR,NDI\params\PSMode\enum,1,,"Disable"
 HKR,NDI\params\PSMode\enum,2,,"Always Enable"
 HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
 HKR,NDI\params\PSMode,optional,0,1

[COMMON.reg]
 HKR,                   ,PRISMIOC               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

 HKR,defaults,ListenInterval,0,3
 HKR,NDI\params\ListenInterval,,0,3
 HKR,Ndi\params\ListenInterval,default,0,3
 HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
 HKR,NDI\params\ListenInterval,type,,int
 HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
 HKR,NDI\params\ListenInterval,min,0,0
 HKR,NDI\params\ListenInterval,max,0,77
 HKR,NDI\params\ListenInterval,step,0,1
 HKR,NDI\params\ListenInterval,optional,0,1

 HKR,defaults,RTSThresh,0,2432
 HKR,NDI\params\RTSThresh,,0,2432
 HKR,Ndi\params\RTSThresh,default,0,2432
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
 HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2432
 HKR,NDI\params\RTSThresh,step,0,64
 HKR,NDI\params\RTSThresh,optional,0,1

 HKR,defaults,FragThresh,0,2432
 HKR,NDI\params\FragThresh,,0,2432
 HKR,Ndi\params\FragThresh,default,0,2432
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
 HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2432
 HKR,NDI\params\FragThresh,step,0,128
 HKR,NDI\params\FragThresh,optional,0,1

 HKR,defaults,PreambleMode,0,1
 HKR,NDI\params\PreambleMode,,0,1
 HKR,Ndi\params\PreambleMode,default,0,1
 HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
 HKR,NDI\params\PreambleMode,type,,enum
 HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
 HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
 HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
 HKR,NDI\params\PreambleMode,optional,0,1

 HKR,defaults,AuthentAlg,0,65535
 HKR,NDI\params\AuthentAlg,,0,65535
 HKR,NDI\params\AuthentAlg,default,0,65535
 HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
 HKR,NDI\params\AuthentAlg,type,,enum
 HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
 HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
 HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
 HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
 HKR,NDI\params\AuthentAlg,optional,0,1

 HKR,defaults,AdhocDemoMode,0,0
 HKR,NDI\params\AdhocDemoMode,,0,0
 HKR,Ndi\params\AdhocDemoMode,default,0,0
 HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
 HKR,NDI\params\AdhocDemoMode,type,,enum
 HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
 HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
 HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
 HKR,NDI\params\AdhocDemoMode,optional,0,1

 HKR,,SSID,0,"default"
 HKR,,DSChannel,0,6

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 PRISM_DRIVER.copy      = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.ME   = 11 ; Win9x=%windir%\system
 PRISM_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[PRISM_NDI.copy]
; PRISMR16.dll           ; Win9x NDI
; PRISMCFG.dll           ; Win9x NDI

[PRISM_NDI.copy.ME]
; PRISMR16.dll           ; Win9x NDI
; PRISMCFG.dll           ; Win9x NDI

[PRISM_COINSTALL.copy.NT]
; PRISMRES.dll
; PRISMIOC.dll
; PRISMCFG.cpl           ; Win2k CoInstaller
; FIXME - Add context sensitive help
;PRISMCFG.hlp           ; Help file
;PRISMCSH.dll           ; Context Sensitive Helper

[PRISM_DRIVER.copy]
; PRISMNDS.sys
; PRISMUSB.sys
; PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.ME]
; PRISMNDS.sys
; PRISMUSB.sys
; PRISMIOC.vxd           ; Win9x Ioctl interface

[PRISM_DRIVER.copy.NT]
; PRISMNDS.sys
; PRISMUSB.sys

[PRISM_APPLET.copy]
; PRISMRES.dll
; PRISMIOC.dll
; PRISMCFG.cpl
; PRISMSTA.exe
; FIXME - Add context sensitive help
;PRISMCFG.hlp           ; Help file
;PRISMCSH.dll           ; Context Sensitive Helper

[PRISM_APPLET.copy.ME]
; PRISMRES.dll
; PRISMIOC.dll
; PRISMCFG.cpl
; PRISMSTA.exe
; FIXME - Add context sensitive help
;PRISMCFG.hlp           ; Help file
;PRISMCSH.dll           ; Context Sensitive Helper

[PRISM_APPLET.copy.NT]
;PRISMRES.dll           ; Copied by coinstaller
;PRISMIOC.dll           ; Copied by coinstaller
;PRISMCFG.cpl           ; Copied by coinstaller
;PRISMCFG.hlp           ; Copied by coinstaller
;PRISMCSH.dll           ; Copied by coinstaller
; PRISMSTA.exe

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
; PRISMR16.dll           = 1,win9x
; PRISMCFG.dll           = 1,win9x
; PRISMIOC.vxd           = 1,win9x
; PRISMRES.dll           = 1
; PRISMIOC.dll           = 1
; PRISMCFG.cpl           = 1,winnt
; PRISMNDS.sys           = 1
; PRISMUSB.sys           = 1
; PRISMSTA.exe           = 1
; FIXME - Add context sensitive help
;PRISMCFG.hlp           = 1
;PRISMCSH.dll           = 1

[SourceDisksFiles.ME]   ; WinMe
; PRISMR16.dll           = 1,win9x
; PRISMCFG.dll           = 1,win9x
; PRISMIOC.vxd           = 1,win9x
; PRISMRES.dll           = 1
; PRISMIOC.dll           = 1
; PRISMCFG.cpl           = 1,winnt
; PRISMNDS.sys           = 1
; PRISMUSB.sys           = 1
; PRISMSTA.exe           = 1
; FIXME - Add context sensitive help
;PRISMCFG.hlp           = 1
;PRISMCSH.dll           = 1

[SourceDisksFiles.X86]  ; Win2k/Xp
; PRISMRES.dll           = 1
; PRISMIOC.dll           = 1
; PRISMCFG.cpl           = 1,win2k
; PRISMNDS.sys           = 1,winxp
; PRISMUSB.sys           = 1,winxp
; PRISMSTA.exe           = 1
; FIXME - Add context sensitive help
;PRISMCFG.hlp           = 1
;PRISMCSH.dll           = 1

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 VER_VENDOR_STR         = "D-Link"
 VER_VENDOR_NAME_STR    = "D-Link Corporation"

 PRISM_PCI1_STR         = "D-Link DWL-520 Wireless PCI Adapter"
 PRISM_PCI2_STR         = "D-Link DWL-520 Wireless PCI Adapter" 
 PRISM_USB1_STR         = "D-LINK DWL-120 WIRELESS USB ADAPTER"

 PRISM_SERVICE_DISPLAY  = "D-Link Wireless LAN Driver"
 PRISM_USB_SERVICE_DISPLAY  = "D-Link Wireless LAN USB Driver"
 INSTALL_DISK_STR       = "D-Link Wireless LAN Install Disk"

 ADHOC_DEMO_STR         = "Adhoc Demo Mode"
 SHORT_PREAM_STR        = "Preamble Mode"
 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 AUTHENT_TYPE_STR       = "Authentication Algorithm"
 LISTENINTERVAL_STR     = "Listen Interval"
 POWER_SAVE_STR         = "Power Save Mode"
 POWER_LEVEL_STR        = "Power Save Level"

